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RICERCA CHIMICA   Electrochemical Division    INOX SYSTEM MAKE UP
THE TECHNOLOGICAL REVOLUTION for the treatment on STAINLESS Steel
NON DANGEROUS PRODUCTS FOR THE OPERATOR: The Unique high-performance System in the world, able to cover the whole treatment cycle on Stainless Steel: degreasing, pickling, passivation, deoxidation (for maintenance)   

Hereby follows the list of 14 VERY IMPORTANT points, to be used when confronting our INOX SYSTEM MAKE UP (ISMU) with Pickling  GEL vary dangerous used within the Golf Area: 
1) INOX SYSTEM MAKE UP can work also under direct sunlight! The gels can't do this, because otherwise they will leave BLACK STAINS on the metal.

Black stains left by the pickling GEL
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2) to avoid the black stains the GEL would leave because of heat, Customers in your area leave the GEL on the metal surface for a very short time. This means that the PICKLING REACTION DOES NOT TAKE PLACE, stopping at just a mild deoxidation. Therefore, CORROSION and PITTING PHENOMENA will appear later on, after the wares have been installed, compromising the whole Plant functionally. PITTING creates cavities, dissolving metal, and because of that, they compromise the structural integrity of the whole installation.
Some Pictures of Severe Problems caused by Pickling GEL
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3) the recent laws in Saudi Arabia and UAE make Pollution containment MANDATORY. Very severe penalties are imposed for the pollution of soil, atmosphere, and water streams and reserves. 
4) the treatment happens instantaneously, whereas GELS and BATHS require time to react. Moreover, GELS require a longer time for rinsing with water after the reaction, compared to the INOX SYSTEM MAKE UP. The rinsing waters generated rinsing GELS must be VERY CAREFULLY contained, since they are extremely contaminating for soil, atmosphere, and water streams and reserves. All these passages cost MONEY that must be added to the cost of the GEL. 
5) INOX SYSTEM MAKE UP uses liquids that are completely NONDANGEROUS! Chemical Products used for treatments of  degreasing, pickling, passivation, deoxidation are not subject to special regulations on transport by road, by sea, by air.

6) With INOX SYSTEM MAKE UP, you can work outside, in the SUN, even in SUMMER!
7) INOX SYSTEM MAKE UP can work on both STAINLESS STEEL and ALUMINUM; in the case of the latter alloys, it works both BEFORE the welding (for a deoxidation that doesn't change the surface finishing, allowing the metal to be welded with considerably LESS HEAT), and AFTER the welding (for a proper PICKLING)
8) INOX SYSTEM MAKE UP works on both big and small surfaces, 24 hours a day, 7 days a week. 
9) INOX SYSTEM MAKE UP allows 2 workers to use one unit at the same time; 
10) it is possible to choose among 14 preloaded programs for all the treatments __ Electro-Degreasing __Electro-Pickling __Passivation __ Electro-branding __Electro-Blackening for artistic finishing. 
11) INOX SYSTEM MAKE UP works with cables that can be prolonged all way up to 32 meters. 
12) INOX SYSTEM MAKE UP allows the use of tools that range from the size of a single brush (for small surfaces), all way up to 350 mm of width (for example, for the whole treatment of big TANKS and VESSELS). This removes the need to SPRAY a dangerous product, and the RISK to contaminate the soil and hurt other workers, and spares the MONEY required to build a containment room.
13) every kind of wares (Pipelines, Vessels, Stairs, Tanks, Tubes, etc.) properly treated by our SYSTEM results to be compliant with International ASTM Standards concerning the Standard Quality of the Resistance against corrosion and pitting. This means that the User can show certificates of compliance with: __ASTM A967 __ASTM B117 __ASTM G48_ ASTM G61

14) Please check how easy becomes the JOB in the following links to online VIDEOS! 
· Video Maintenance/elimination of existing corrosion using NON Dangerous products https://ricercachimica.it/canale-inox/#videoItem-16   

· Video of Pickling using NON-Dangerous products https://ricercachimica.it/canale-inox/#videoItem-21    

· Video of Pickling inside a tank using NON-Dangerous products  https://ricercachimica.it/canale-inox/#videoItem-33 
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